1. PRODUCTS
	1. MANUFACTURERS
		1. Contract Documents are based on Pinnacle workstations by Winsted, [www.winsted.com](http://www.winsted.com).
		2. Substitutions: [Refer to Division 01.] [Not permitted.]
	2. COMPONENTS
		1. Frame:
			1. Type: [Pinnacle 60”.] [Pinnacle 72”.] [Pinnacle 84”.] [Pinnacle 96”.]
			2. Material: Steel.
		2. Base:
			1. Closed height adjustable: [Pinnacle 60”.] [Pinnacle 72”.] [Pinnacle 84”.] [Pinnacle 96”.]
		3. Work Surface:
			1. Type: Single
			2. Construction: [1-1/8 inch thick medium density fiberboard with laminate facings.] [5/8 inch thick compact laminate.]
			3. Faces: laminate
			4. Edge type: [Safeguard plus, 1-1/8 inch black polyethylene T-edge, routed into edge.] [Exposed core.] [Comfort Edge, 1-1/8 inch molded urethane shaped edge.]
			5. Laminate face color:
		4. End Panels:
			1. Core material: [1/2 inch thick medium density fiberboard with laminate facings.] [1/2 inch thick compact laminate.]
			2. Faces: laminate
			3. Laminate face color:
			4. Laminate grain direction:
				1. Work surfaces: Along length of component.
				2. Doors and end panels: [Horizontal.] [Vertical.]
		5. Doors:
			1. Construction: [Ventilated Steel.] [3/4 inch thick medium density fiberboard with laminate facings.]
			2. Faces: laminate
			3. Laminate face color: [White.] [Black.] [Gray.] [Maple.] [Walnut.] [\_\_\_\_.]
			4. Latches: Soft touch type.
		6. Lifting Columns: Two sets of two columns.
		7. Power Compatibility: 110V and 240V capable; hardwire ready duplex power.
		8. Versa-Trak: Provide infinite monitor arm adjustability.
		9. Cable Management:
			1. Technology tray: reveled by sliding/lockable worksurface
			2. Cable Management Trays: 3 full length continuous trays (Top/Bottom/ Worksurface)
		10. Accessories:
			1. CPU pedestals.
			2. Monitor mounts and mounting posts.
			3. Phone trays.
			4. Laptop trays.
			5. Keyboard trays.
			6. Pro Series II racks.
			7. Surface mounted Qi Wireless Phone Charging
			8. Bi-Directional Slide-Out Rotating PC Tray
			9. Under worksurface mounted drawers
			10. Ethernet Tripp Lite Patch Panel
	3. FINISHES
		1. Steel: Manufacturer’s standard black powder coat.
		2. Aluminum: Silver anodized.